| Home > Product Information Technical Specifications Paper Memory Card Slots Ink Cartridges Mechanical Electrical Environmental Standards and Approvals USB Interface Paper
| Note:
Since the quality of any particular brand or type of paper may be changed by the manufacturer at any time, Epson cannot attest to the quality of any non-Epson brand or type of paper. Always test samples of paper stock before purchasing large quantities or printing large jobs.
Single sheets:
Size | A4 210 × 297 mm 10 × 15 cm (4 × 6 in) 13 × 18 cm (5 × 7 in) A6 105 × 148 mm A5 148 × 210 mm B5 182 × 257 mm 9 × 13 cm (3.5 × 5 in) 13 × 20 cm (5 × 8 in) 20 × 25 cm (8 × 10 in) Letter 8 1/2 × 11 in Legal 8 1/2 × 14 in
Paper types | Plain bond paper or special paper distributed by Epson
Thickness (for plain bond paper) | 0.08 to 0.11 mm (0.003 to 0.005 in)
Weight (for plain bond paper) | 64g/m² (17lb) to 90g/m² (24lb)
Envelopes:
Size | Envelope #10 4 1/8 × 9 1/2 in Envelope DL 110 × 220 mm Envelope C6 114 × 162 mm Envelope 132 × 220 mm
Paper types | Plain bond paper, Air Mail
Weight | 75g/m² (20lb) to 90g/m² (24lb)
| Note:
Poor quality paper may reduce print quality and cause paper jams or other problems. If you encounter problems, switch to a higher grade of paper. Do not load curled or folded paper. Use paper under normal conditions: Temperature 15 to 25 ˚C (59 to 77 ˚F) Humidity 40 to 60% RH
Printable area Single sheets and index cards:
Normal | Borderless
Envelopes:
Diagonal lines show printable area.
A: | The minimum top margin is 3.0 mm (0.12 in).
B-L: | The minimum left margin is 3.0 mm (0.12 in). The minimum left margin is 5.0 mm (0.20 in) for envelopes.
B-R: | The minimum right margin is 3.0 mm (0.12 in). The minimum right margin is 5.0 mm (0.20 in) for envelopes.
C: | The minimum bottom margin is 20 mm (0.78 in) for single sheets and index cards.
| Note:
Depending on the type of paper, print quality may decline in the top and bottom areas of the printout, or the area may be smeared.
Top Memory Card Slots
Compatible memory cards | CompactFlash SmartMedia* Memory Stick Memory Stick PRO Memory Stick Duo** Memory Stick PRO Duo** MagicGate Memory Stick MagicGate Memory Stick Duo** Microdrive SD (Secure Digital) Card MultiMediaCard miniSD Card** xD-Picture Card xD-Picture Card Type M
Voltage Requirements | 3.3 v Maximum current is 500 mA
* Maximum capacity is 128 MB. ** Adapter required. Memory card slot compatibility:
CF Type II card slot | Compatible with CF+ and CompactFlash Specification 1.4 cards
SmartMedia card slot | Compatible with SmartMedia Standard 2003 cards
Memory Stick/MemoryStick PRO card slot | Compatible with Memory Stick Standard version 1.3 or Memory Stick Standard Memory Stick PRO Format Specifications version 1.0 cards
SD/MMC card slot | Compatible with SD Memory Card Specifications / PART1. Physical Layer Specification Version 1.0 cards and MultiMediaCard Standard cards
xD-Picture card Slot | Compatible with xD-Picture Card™ Card Specification Version 1.20 Type M cards
Top Ink Cartridges
Color | Yellow, Magenta, Cyan, Light Magenta, Light Cyan, Black
Cartridge life | Within 6 months of opening the package at 25 ˚C [77 ˚F]
Temperature | Storage: -20 to 40 ˚C (-4 to 104 ˚F) 1 month at 40 ˚C (104 ˚F) Freezing:* -18 ˚C (-0.4 ˚F)
Dimensions | 12.7 mm (W) × 73.5 mm (D) × 55.3 mm (H)
* Ink thaws and is usable after approximately 3 hours at 25 ˚C (77 ˚F).
| Caution:
Epson recommends the use of genuine Epson ink cartridges. Epson warranties do not cover damage to this product caused by the use of ink cartridges not manufactured by Epson. Do not use an ink cartridge if the date on the package has expired. Do not refill the ink cartridge. This product calculates the amount of ink remaining using an IC chip on the ink cartridge, so even if the cartridge is refilled, the IC chip will report that it is empty.
| Note:
The ink cartridges packaged with your printer are partly used during initial setup. In order to produce high quality printouts, the print head in your printer will be fully charged with ink. This one-off process consumes a quantity of ink and subsequent cartridge sets will last for their full rated life.
Top Mechanical
Paper path | Sheet feeder, top entry
Sheet feeder capacity | About 120 sheets at 90 g/m² (24 lb) paper
Dimensions | Storage Width: 483 mm (19.0 inches) Depth: 300 mm (11.8 inches) Height: 188 mm (7.4 inches)
Printing Width: 483 mm (19.0 inches) Depth: 478 mm (18.8 inches) Height: 297 mm (11.7 inches)
Weight | 6.1 kg (13.4 lb) without the ink cartridges
Top Electrical
| 120V Model | 220-240V Model
Input voltage range | 99 to132 V | 198 to 264 V
Rated frequency range | 50 to 60 Hz
Input frequency range | 49.5 to 60.5 Hz
Rated current | 0.4A (Max. 0.7 A) | 0.2A (Max. 0.4 A)
Power consumption | Approx. 13 W (ISO10561 Letter Pattern) Approx. 2.2 W in Sleep mode Approx. 0.2 W in Power Off mode | Approx. 13 W (ISO10561 Letter Pattern) Approx. 2.3 W in Sleep mode Approx. 0.3 W in Power Off mode
| Note:
Check the label on the back of the printer for its voltage.
Top Environmental
Temperature | Operation: 10 to 35 ˚C (50 to 95 ˚F) Storage: -20 to 40 ˚C (-4 to 104 ˚F) 1 month at 40 ˚C (104 ˚F)
Humidity | Operation: * 20 to 80% RH Storage:* 5 to 85% RH
* Without condensation Top Standards and Approvals U.S. model:
Safety | UL 60950 CSA 22.2 No.950
EMC | FCC Part 15 Subpart B Class B CAN/CSA-CEI/IEC CISPR 22 Class B
European model:
Low voltage directive 73/72/EEC | EN 60950
EMC directive 89/336/EEC | EN55022 Class B EN61000-3-2 EN61000-3-3 EN55024
Australian model:
EMC | AS/NZS CISPR22 Class B
Top USB Interface
Standard | Based on Universal Serial Bus Specifications Revision 2.0, Universal Serial Bus Device Class Definition for Printing Devices Version 1.1, Universal Serial Bus Mass Storage class Bulk-Only Transport Revision 1.0
Bit rate | 480 Mbps (High speed device)
Data encoding | NRZI
Adaptable connector | USB Series B
Recommended cable length | Under 2 meters
Top |