| Home > Using the Optional Bluetooth Adapter Setting the Bluetooth Passkey (Bluetooth PIN) If you select Pairing as the Communication Mode or turn on encryption, you must enter a Passkey into your Bluetooth-enabled device before it can communicate with the printer. The default Passkey is 0000. To change the Passkey, follow these steps:
| Press the Setup button.
| Press the or button to highlight BT PIN Code Set, then press the button.
| Press the or button to select a number for the first digit, then press the button.
| Repeat step 3 for the second through fourth digits.
| Press the OK button to activate the Passkey.