| Home > Using the Optional Bluetooth Adapter Choosing Bluetooth Settings If necessary, use your printer’s LCD panel to select settings for Bluetooth wireless communication. You may need to enter a passkey for your printer or turn on encryption, depending on the settings for the Bluetooth-enabled device.
| Press the or buttons and the button to select settings as listed in the following table.
Menu item | Settings | Description
BT Printer ID Set | printer name- (number) (Default = 1) | If multiple Bluetooth-enabled printers are in the same communication range, assign a number from 0 through 9 to each printer. To make the Device Name Setting take effect, turn the printer off and then back on.
BT Connectivity Mode | Discoverable | This mode allows Bluetooth-enabled devices to freely discover the printer and send print jobs.
Not Discoverable | This mode prevents unknown devices from discovering the printer. To print in "Not Discoverable" mode, first search for the printer in "Discoverable" mode. After your device has discovered the printer in "Discoverable" mode, it will subsequently be able to communicate with it and print in "Discoverable" mode.
Pairing | This mode requires you to enter a four-digit Passkey into a device before it can communicate with the printer.
BT Encryption | On/Off (Default = Off) | Select On to encrypt communication. Encryption requires you to enter the four-digit Passkey into a device before it can communicate with the printer.
BT PIN Code Set | Any four-digit number (Default = 0000) | The Passkey Setting allows you to set the four-digit Passkey required for Bonding or Encryption.
BT Device Address | Set at the factory (Example) 11-11-11-11-11-11 | Displays the unique Bluetooth Device Address of the printer.