How to Use EPSON Paper Feed Adjuster

# Paper Feed Adjustment Detail

Set Paper Feed Adjustment values and make sample prints.

Adjusts the paper feed value in 0.01% increments. If the paper feed value is too large, white horizontal micro-banding may appear. If the paper feed value is too small, dark horizontal micro-banding may appear.

To eliminate banding, set the Test Range by using the slider, or enter a value in the text box. To remove white banding, move the slider toward - 25. To remove dark banding, move the slider toward + 25.

| Note:

The value of each unit is 0.01%. Therefore, you can specify a maximum offset of ± 0.25% from the default paper feed value.

| Set the minimum and maximum values to determine the range by using the sliders or text boxes.

|  | Note:

Between the minimum and maximum values, five values are determined for the sample feed value. These five values are displayed above the Sample Prints button.

| To use a specific image as the sample print for choosing the most appropriate media, select User Defined Image, then click the Browse button to find the image.

|  | Note:

EPSON recommends selecting Standard Image for Sample Prints.

The allowable size for the User Defined Image must be within 3060 x 425 pixels and must be in 24-bit BMP file format.

> To use a standard image, select the corresponding option.

| Click the Sample Prints button.

| In the Page Setup dialog box, select On or Off for Auto Cut, then select Paper Size in the list box. When you select On for Auto Cut, the printed sheet is cut automatically.

| Click OK if you approve of the information in the Sample Print dialog box.

| Look over the samples and determine which image has the least amount of banding. A value is printed next to each image.

| Repeat steps 1 through 6 until banding is eliminated.

| Enter the value you determined in the Adjustment Value text box.

| Click Save.

| Click Close.

[Top]

Previous | Next