Other Information

# Loading Single Sheets of Paper

Follow the steps below to load paper into the printer.

| Open the paper support, then slide out the extension.

| Make sure that the output tray is down and slide out the extension.

| Changing the Position of the Output Tray

| Position the left edge guide so that the distance between the two edge guides is slightly wider than the width of your paper.

| Fan a stack of paper, then tap it on a flat surface to even the edges.

| Load the paper with the printable side up so it is against the right edge guide, and slide it into the sheet feeder. Then slide the left edge guide against the left edge of the paper.

|  | Note:

Leave enough space in front of the printer for the paper to be fully ejected.

Always load paper into the sheet feeder short edge first.

Make sure that the paper stack is flush with or lower than the triangular load-limit mark on the edge guide.

[Top]

Previous | Next