# Safety Instructions

> When setting up your printer
> When choosing a place for the printer
> When using the printer
> When handling the ink cartridges
> Information for United Kingdom Users
> Warnings, Cautions, and Notes

| Read all of the instructions in this section before using your printer. Also, be sure to follow all warnings and instructions marked on the printer. ## When setting up your printer Observe the following when setting up the printer: Do not block or cover the vents and openings in the printer. Use only the type of power source indicated on the printer's label. Use only the power cord that comes with this product. Use of another cord may result in fire or electric shock. This product's power cord is for use with this product only. Use with other equipment may result in fire or electric shock. Be sure your AC power cord meets the relevant local safety standards. Avoid using outlets on the same circuit as photocopiers or air control systems that regularly switch on and off. Avoid using electrical outlets controlled by wall switches or automatic timers. Keep the entire computer system away from potential sources of electromagnetic interference, such as loudspeakers or the base units of cordless telephones. Do not use a damaged or frayed power cord. If you use an extension cord with the printer, make sure that the total ampere rating of the devices plugged into the extension cord does not exceed the cord's ampere rating. Also, make sure that the total ampere rating of all devices plugged into the wall outlet does not exceed the wall outlet's ampere rating. Do not attempt to service the printer yourself. Unplug the printer and refer servicing to qualified service personnel under the following conditions: The power cord or plug is damaged; liquid has entered the printer; the printer has been dropped or the casing damaged; the printer does not operate normally or exhibits a distinct change in performance. If you plan to use the printer in Germany, the building installation must be protected by a10 or 16 amp circuit breaker to provide adequate short-circuit protection and over-current protection for this printer.
|  | Note for German-speaking users:
Bei Anschluss des Druckers an die Stromversorgung muss sichergestellt werden, dass die Gebäudeinstallation mit einer 10 A- oder 16 A-Sicherung abgesichert ist.
## When choosing a place for the printer Observe the following when choosing a place for the printer: Place the printer on a flat, stable surface that extends beyond the base of the printer in all directions. If you place the printer by the wall, leave more than 10 cm between the back of the printer and the wall. The printer will not operate properly if it is tilted at an angle. When storing or transporting the printer, do not tilt it, stand it on its side, or turn it upside down. Otherwise, ink may leak from the cartridges. Leave enough space in front of the printer for the paper to be fully ejected. Avoid places subject to rapid changes in temperature and humidity. Also, keep the printer away from direct sunlight, strong light, or heat sources. Avoid places subject to dust, shock, or vibration. Leave enough room around the printer to allow for sufficient ventilation. Place the printer near a wall outlet where the plug can be easily unplugged.
|  | Note for French-speaking users:
Placez l'imprimante près d'une prise de contacte où la fiche peut être débranchée facilement.
## When using the printer Observe the following when using the printer: Do not insert objects through the slots in the printer. Take care not to spill liquid on the printer. Do not put your hand inside the printer or touch the ink cartridges during printing. Do not move the print head by hand; otherwise, you may damage the printer. Always turn the printer off using the power button. When this button is pressed, the power light flashed. Do not unplug the printer or turn off the power to the outlet until the power light stops flashing. Before transporting the printer, make sure that the print head is in the home (far right) position and the ink cartridges are in place. Leave the ink cartridges installed. Removing the cartridges can dehydrate the print head and may prevent the printer from printing. ## When handling the ink cartridges Observe the following when handling the ink cartridges: Keep ink cartridges out of the reach of children. Do not allow children to drink from or otherwise handle the cartridges. Shake the new ink cartridges four or five times before opening the packages. Do not shake the ink cartridges after opening the pakcages; this can cause leakage. Be careful when you handle used ink cartridges, as there may be some ink remaining around the ink supply port. If ink gets onto your skin, wash the area thoroughly with soap and water. If ink gets into your eyes, flush them immediately with water. If discomfort or vision problems continue after a thorough flushing, see a doctor immediately. Do not remove or tear the label on the cartridge; this can cause leakage. Install the ink cartridge immediately after you remove it from its package. If you leave a cartridge unpacked for a long time before using it, normal printing may not be possible. Do not use an ink cartridge beyond the date printed on the cartridge carton: otherwise, it may result in reduced print quality. For best results, use up the ink cartridges within six months of first installing them. Do not dismantle the ink cartridges or try to refill them. This could damage the print head. After bringing an ink cartridge inside from a cold storage site, allow it to warm up at room temperature for at least three hours before using it. Store ink cartridges in a cool, dark place. Do not touch the green IC chip on the back of the cartridge. Doing so may prevent normal operation and printing. The IC chip on this ink cartridge retains a variety of cartridge-related information, such as the amount of ink remaining, so that the cartridge may be removed and reinstalled freely. However, each time the cartridge is inserted, some ink is consumed because the printer automatically performs a reliability check. If you remove an ink cartridge for later use, protect the ink supply area from dirt and dust and store it in the same environment as the printer. A valve in the ink supply port makes covers or plugs unnecessary, but the ink may stain items that come into contact with this area of the cartridge. Do not touch the ink supply port or the surrounding area. Store ink cartridge with its label facing upward. Do not store cartridge upside down. ### ENERGY STAR® Compliance As an ENERGY STAR® Partner, Epson has determined that this product meets the ENERGY STAR® guidelines for energy efficiency. The International ENERGY STAR® Office Equipment Program is a voluntary partnership with the computer and office equipment industry to promote the introduction of energy-efficient personal computers, monitors, printers, fax machines, copiers, scanners, and multifunction devices in an effort to reduce air pollution caused by power generation. Their standards and logos are uniform among participating nations. ## Information for United Kingdom Users ### Use of options EPSON (UK) Limited shall not be liable against any damages or problems arising from the use of any options or consumable products other than those designated as Original EPSON Products or EPSON Approved Products by EPSON (UK) Limited. ### Safety information
| Warning:
Refer to the rating plate for the voltage and check that the appliance voltage corresponds to the supply voltage. Important: The wires in the mains lead fitted to this appliance are coloured in accordance with the following code: Blue — Neutral Brown — Live
If you have to fit a plug: As the colours of the mains lead of this appliance may not match the coloured markings used to identify the terminals in a plug, please observe the following: The blue wire must be connected to the terminal in the plug marked with the letter N. The brown wire must be connected to the terminal in the plug marked with the letter L. If the plug is damaged, replace the cord set or consult a qualified electrician. Replace fuses only with fuses of the correct size and rating. ## Warnings, Cautions, and Notes
| Warnings
must be followed carefully to avoid bodily injury.
| Cautions
must be observed to avoid damage to your equipment.
| Notes
contain important information and useful tips on the operation of your printer.