Various Printing Options

# Double-Sided Printing

> Standard double-sided printing for Windows
> Standard double-sided printing for Macintosh
> Folded Booklet double-sided printing for Windows
> Folded Booklet double-sided printing for Macintosh

There are two types of double-sided printing available. Standard double-sided printing allows you to print the odd-numbered pages first. Once these pages are printed, they can be reloaded to print the even-numbered pages onto the opposite side of the paper.

Folded Booklet double-sided printing allows you to make single-fold booklets. To create it, the pages that appear on the outside (after the page is folded) are printed first. The pages that will appear inside the booklet can then be printed after the paper is reloaded into the printer as shown in the illustration below.

| Single-fold booklet

| : Binding edge

A booklet can be created by printing pages 1 and 4 on the first sheet of paper, pages 5 and 8 on the second sheet of paper, and pages 9 and 12 on the third sheet of paper. After these sheets are reloaded into the sheet feeder, you can then print pages 2 and 3 on the back of the first sheet of paper, pages 6 and 7 on the back of the second sheet of paper, and pages 10 and 11 on the back of the third sheet of paper. The resulting pages can then be folded and bound together into a booklet.

| Note:

This feature is not available with Mac OS X.

This feature is not available when selecting the Borderless check box on the Main menu (Windows) or in the Page Setup dialog box (Macintosh).

This feature is not available when the printer is accessed over a network or is used as a shared printer.

Depending on the media type, stacks of up to 30 sheets can be loaded into the sheet feeder during double-sided printing.

Only use media types that are suitable for double-sided printing. Otherwise, the printout quality may deteriorate.

Depending on the media type and the amount of ink used to print text and images, ink may bleed through to the other side of the paper.

The surface of the paper may be smeared during double-sided printing.

## Standard double-sided printing for Windows

Follow the steps below to print odd- and even-numbered pages onto opposite sides of the sheet.

| Access the printer driver.

| Accessing the Printer Software for Windows

| Click the Main tab, then make the Quality Option setting. See the following section for details on the Quality Option settings. See Quality Option

| Select Sheet as the Source setting.

| Make the appropriate Type setting.

| Media Type Settings

| Make the appropriate Size setting.

| Click the Page Layout tab, then select the Double-Sided Printing check box.

| Click Margins to open the Margins dialog box.

| Specify the edge of the paper where the binding will be placed. You can choose Left, Top, or Right.

| Choose cm or inch as the Unit setting. Then, specify the width of the binding margin. You can enter any width from 0.3 cm to 3.0 cm, or from 0.12 inches to 1.18 inches.

|  | Note:

The actual binding margin may be different from the specified settings depending on your application. Experiment with a few sheets to examine actual results before printing the entire job.

| Click OK to return to the Page Layout menu. Then, click OK to save your settings.

| Load paper into the sheet feeder, then send the print job from your application. Instructions for generating the even-numbered pages will be displayed while the odd-numbered pages are printed.

| Loading Single Sheets of Paper

| Follow the on-screen instructions to reload the paper.

|  | Note:

The paper may curl during printing due to the amount of ink used. Should this occur, slightly curl the sheets in the opposite direction before reloading them into the printer.

Align the sheet stack by tapping its edges against a hard, flat surface before reloading the stack into the printer.

Follow the instructions provided when reloading the printouts. Paper jams or improperly placed binding margins may occur if the printouts are not reloaded correctly.

If a paper jam occurs, refer to the following. See Paper Does Not Feed Correctly

| Once the paper is reloaded, click Resume to print the even-numbered pages.

[Top]

## Standard double-sided printing for Macintosh

Follow the steps below to print odd- and even-numbered pages onto opposite sides of the sheet.

| Access the Page Setup dialog box.

| Accessing the Printer Software for Mac OS 8.6 to 9.x

| Make the appropriate Paper Size setting.

| Select Auto Sheet Feeder as the Paper Source.

| Select the Double-Sided Printing check box.

| Click Margins.

| Specify the edge of the paper where the binding will be placed. You can choose Left, Top, or Right.

| Specify the width of the binding margin in the text box. You can enter any width from 0.12 inch to 1.18 inch or from 0.3 cm to 3.0 cm.

|  | Note:

The actual binding margin may be different from the specified settings depending on your application. Experiment with a few sheets to examine actual results before printing the entire job.

| Click OK to return to the Page Setup dialog box. Then, click OK to save your settings and close the dialog box.

| Access the Print dialog box.

| Accessing the Printer Software for Mac OS 8.6 to 9.x

| Make the appropriate Media Type setting.

| Media Type Settings

| Load paper into the sheet feeder, then click Print to start printing. Instructions for generating the even-numbered pages will be displayed while the odd-numbered pages are printed.

| Loading Single Sheets of Paper

| Follow the on-screen instructions to reload the paper.

|  | Note:

The paper may curl during printing due to the amount of ink used. Should this occur, slightly curl the sheets in the opposite direction before reloading them into the printer.

Align the sheet stack by tapping its edges against a hard, flat surface before reloading the stack into the printer.

Follow the instructions provided when reloading the printouts. Paper jams or improperly placed binding margins may occur if the printouts are not reloaded correctly.

If a paper jam occurs, refer to the following. See Paper Does Not Feed Correctly

| Once the paper is reloaded, click Resume to print the even-numbered pages.

[Top]

## Folded Booklet double-sided printing for Windows

Use the following steps to create a folded booklet as described in the beginning of this section.

| Access the printer driver.

| Accessing the Printer Software for Windows

| Click the Main tab, then make the Quality Option setting. See the following section for details on the Quality Option settings. See Quality Option

| Select Sheet as the Source setting.

| Make the appropriate Type setting.

| Media Type Settings

| Make the appropriate Size setting.

| Click the Page Layout tab and select the Double-Sided Printing check box. Then, select the Folded Booklet check box.

| Click Margins to open the Margins dialog box.

| Specify the edge of the paper where the binding will be placed. You can choose Left, Top, or Right.

|  | Note:

When Portrait is selected as the Orientation setting on the Main menu, the Left or Right binding positions are available. The Top binding position is available when Landscape is selected as the Orientation setting.

| Choose cm or inch as the Unit setting. Specify the width of the binding margin. You can enter any width from 0.3 cm to 3.0 cm, or from 0.12 inches to 1.18 inches. The specified margin width will be used on both sides of the fold. For example, if a 10-mm margin is specified, a 20-mm margin will be inserted (a margin of 10 mm will be placed on each side of the fold).

Portrait | Landscape

| : Folding edge

| : Margin

| Click OK to return to the Page Layout menu. Then, click OK to save your settings.

| Load paper into the sheet feeder, then send the print job from your application. Instructions for printing the inside pages will be displayed while the outside pages are printed.

| Loading Single Sheets of Paper

| Follow the on-screen instructions to reload the paper.

|  | Note:

The paper may curl during printing due to the amount of ink used. Should this occur, slightly curl the sheets in the opposite direction before reloading them into the printer.

Align the sheet stack by tapping its edges against a hard, flat surface before reloading the stack into the printer.

Follow the instructions provided when reloading the printouts. Paper jams or improperly placed binding margins may occur if the printouts are not reloaded correctly.

If a paper jam occurs, refer to the following. See Paper Does Not Feed Correctly

| Once the paper is reloaded, click Resume to print the inside pages.

| Once printing is complete, fold the sheets and bind them together using a stapler or other binding method.

[Top]

## Folded Booklet double-sided printing for Macintosh

Use the following steps to create a folded booklet as described in the beginning of this section.

| Access the Page Setup dialog box.

| Accessing the Printer Software for Mac OS 8.6 to 9.x

| Make the appropriate Paper Size setting.

| Select Auto Sheet Feeder as the Paper Source.

| Select the Double-Sided Printing check box. Then, select the Folded Booklet check box.

| Click Margins.

| Specify the edge of the paper where the binding will be placed. You can choose Left, Top, or Right.

|  | Note:

When Portrait is selected as the Orientation setting in the Page Setup dialog box, the Left or Right binding positions are available. The Top binding position is supported when Landscape is selected as the Orientation setting.

| Specify the width of the binding margin in the text box. You can enter any width from 0.12 inch to 1.18 inch or from 0.3 cm to 3.0 cm.The specified margin width will be used on both sides of the fold. For example, if a 10-mm margin is specified, a 20-mm margin will be inserted (a margin of 10 mm will be placed on each side of the fold).

Portrait | Landscape

| : Folding edge

| : Margin

| Click OK to return to the Page Setup dialog box. Then, click OK to save your settings and close the dialog box.

| Access the Print dialog box.

| Accessing the Printer Software for Mac OS 8.6 to 9.x

| Make the appropriate Media Type setting.

| Media Type Settings

| Load paper into the sheet feeder, then click Print to start printing. Instructions for printing the inside pages will be displayed while the outside pages are printed.

| Loading Single Sheets of Paper

| Follow the on-screen instructions to reload the paper.

|  | Note:

The paper may curl during printing due to the amount of ink used. Should this occur, slightly curl the sheets in the opposite direction before reloading them into the printer.

Align the sheet stack by tapping its edges against a hard, flat surface before reloading the stack into the printer.

Follow the instructions provided when reloading the printouts. Paper jams or improperly placed binding margins may occur if the printouts are not reloaded correctly.

If a paper jam occurs, refer to the following. See Paper Does Not Feed Correctly

| Once the paper is reloaded, click Resume to print the inside pages.

| Once printing is complete, fold the sheets and bind them together using a stapler or other binding method.

[Top]

Previous | Next