How to Use EPSON Paper Feed Adjuster

# Print Current Adjustment Values

Print the current Paper Feed Adjustment and MicroWeave Adjustment values.

Click Print to print current adjustment values. The following sheet is printed.

> a: Adjustment items with some print settings

> b: Marking on the changed value

> c: Media types with various print settings

The printed sheet is shown in the diagram above. The diagram shows the current adjustment values for each media type. If the value was changed, an asterisk (*) is shown next to the value. The letters, A, B, C, and D in the column head refer to adjustment items and print settings in the following ways:

##### A: MicroWeave Adjustment for Advanced Photo and SuperFine-1440 dpi Print Quality

Shows MicroWeave Adjustment values when you print with Advanced Photo or SuperFine-1440 dpi as the print quality.

##### B: MicroWeave Adjustment for Normal-360 dpi and Fine-720 dpi Print Quality

Shows MicroWeave Adjustment values when you print with Normal-360 dpi or Fine-720 dpi as the print quality.

##### C: Paper Feed Adjustment for Roll Paper and Manual Feed

Shows Paper Feed Adjustment values when you print with Roll Paper or Manual Feed as the paper source.

##### D: Paper Feed Adjustment for Paper Tray

Shows Paper Feed Adjustment values when you print with Paper Tray as the paper source.

The numbers with the sharp symbol (#) in the row heading are media types combined with various print settings. The number varies depending on the media type, the resolution setting, the paper source, and so on. This number corresponds to the number shown next to options in the Media Type list box in the Adjustments dialog box.

[Top]

Previous | Next