Other Information / Printer Specifications

# Electrical

| 120 V Model | 220-240 V Model
Input voltage range | 99 to 132 V | 198 to 264 V
Rated frequency range | 50 to 60 Hz
Input frequency range | 49.5 to 60.5 Hz
Rated current | 0.5 A (Max. 0.8 A) | 0.25 A (Max. 0.4 A)
Power consumption | Approx. 20 W (ISO10561 Letter Pattern) Approx. 2 W in Sleep mode | Approx. 20 W (ISO10561 Letter Pattern) Approx. 2.5 W in Sleep mode

| Note:

Check the label on the back of the printer for the voltage of your printer.

[Top]

Previous | Next