Other Information

# Printer Parts and Control Panel Functions

> Printer Parts
> Control panel

## Printer Parts

a. Paper support: Supports the paper loaded in the sheet feeder.

b. Sheet feeder: Holds blank paper and automatically feeds the paper during printing.

c. Printer cover: Covers the printing mechanism. Open only when installing or replacing ink cartridges.

d. Output tray extension: Supports the ejected paper.

e. Output tray: Receives the ejected paper.

f. Manual sheet slot: Holds the CD/DVD tray or the matte board and feeds them.

g. Edge guides: Help load the paper straight. Adjust the left edge guide to fit the width of your paper.

a. Roll paper edge guide: Helps load the roll paper straight. Adjust the edge guide to fit the width of your paper.

b. Roll paper feeder: Holds the roll paper and automatically feeds it after holding the roll paper with your hand for three seconds.

c. USB interface cable connector: Used to connect the USB cable to the computer and the printer.

d. IEEE 1394 interface cable connector: Used to connect the IEEE cable to the computer and the printer.

e. Roll paper holder: Attaches to the printer and holds the roll paper.

f. Roll paper knob: Turn to roll up the roll paper.

a. Cartridge cover: Hold the ink cartridges in place. Open only when installing or replacing ink cartridges.

b. Print head: Delivers ink to the page.

c. Control panel: Controls various printer functions. See the next section for details.

[Top]

## Control panel

### Buttons

Button | Function
power | Turns the printer on and off.
paper | Loads or ejects paper. Resumes printing if pressed after a paper out error or double feed error. Cancels the printing of a print job if pressed while printing.
ink | Moves the print head to the ink cartridge replacement position. Move the print head to the ink check position when an empty ink cartridge is detected. Returns the print head to its home position after ink cartridge replacement. Performs print head cleaning if held down for three seconds when the ink out light is off.
roll paper | Prints a cutting guideline and feeds roll paper to a position where it can be easily removed from the sheet feeder if pressed after printing. Feeds roll paper to the printing position if pressed after cutting the paper. Feeds roll paper in reverse to a position where it can be easily removed from the roll paper feeder if pressed for 3 seconds.

### Lights

Light | Description
power | On when the printer is on. Flashing when the printer is receiving data, printing, having an ink cartridge replaced, charging ink, or cleaning the print head.
paper out | On when the printer is out of paper or when the CD/DVD tray is not set. Flashing when the paper or CD/DVD tray is jammed, or when the output tray is in an incorrect position.
ink out | On when an ink cartridge is empty. Flashing when an ink cartridge is nearly empty.

[Top]

Previous | Next